IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "RevitIdentifiers [VersionGUID: f0f73a66-1d87-45e7-a90b-161458927212, NumberOfSaves: 1]"
Description: "CoordinateReference [CoordinateBase: Origem interna, ProjectSite: Terreno padrão]"
File name: "ARC10W.ifc"
Time stamp: "2025-03-06T10:05:00"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.80.32 - IFC 22.7.0.0 - Default UI"
Application: "Autodesk Revit 2022 (PTB)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (PTB)"

People and organizations
  Person "analuiza.dagnoni" of Organization (no name given)
  Owner history of Person "analuiza.dagnoni" of Organization (no name given) | application "Autodesk Revit 2022 (PTB)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (PTB)" | change NOCHANGE | created 1741193024 (2025-03-05T16:43:44Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  ENERGYUNIT: JOULE
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATFLUXDENSITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived
  MASSPERLENGTHUNIT: derived
  THERMALRESISTANCEUNIT: derived
  ACCELERATIONUNIT: derived
  ANGULARVELOCITYUNIT: derived
  LINEARSTIFFNESSUNIT: derived
  WARPINGCONSTANTUNIT: derived
  LINEARMOMENTUNIT: derived
  TORQUEUNIT: derived

Spatial structure
IFCPROJECT "0001" | long name "Nome do projeto" | phase "Status do projeto"
  IFCSITE "Default" | latitude -15° 52′ 0.12062″ | longitude -47° 55′ 0.11444″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Insira aqui o endereço", "Brasília", "Brasil"
      IFCBUILDINGSTOREY "Nível 1" | long name "Nível 1" | object type "Nível:Cabeça de 8 mm" | elevation 0.
        contains 1 element
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "ArandelaConcreto_ARC10W_PowerLume:ARC10W" | object type "ArandelaConcreto_ARC10W_PowerLume:ARC10W" | names: "ArandelaConcreto_ARC10W_PowerLume:ARC10W:326700" | material: materials ("LED", "Metal - Alumínio", "Acrílico - Transparente", "Concreto, leve") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff

Types
  IFCLIGHTFIXTURETYPE "ArandelaConcreto_ARC10W_PowerLume:ARC10W" | 1 occurrence | material: materials ("LED", "Metal - Alumínio", "Acrílico - Transparente", "Concreto, leve") | property sets: Pset_ManufacturerTypeInformation, Fotométrica, Dados de identidade, Materiais e acabamentos, Dados, Elétrica

Property sets
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    Reference = "ArandelaConcreto_ARC10W_PowerLume:ARC10W" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCFLOWTERMINAL)
    Reference = "ArandelaConcreto_ARC10W_PowerLume:ARC10W" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    Manufacturer = "Power Lume" (IFCLABEL)
  Fotométrica | properties | on 1 type object
    Fluxo luminoso = "725 lm" (IFCTEXT)
    IRC = "90" (IFCTEXT)
    Potência = "10W" (IFCTEXT)
    Temperatura de cor = "3000K" (IFCTEXT)
    Ângulo de abertura = "2x80°" (IFCTEXT)
  Dados de identidade | properties | on 1 type object
    Catálogo de produtos = "https://www.powerlume.com.br/downloads" (IFCTEXT)
    Contato do fabricante = "(54) 3066-6488" (IFCTEXT)
    Descrição = "Arandela de sobrepor LED facho direto e indireto em concreto" (IFCTEXT)
    Fabricante = "Power Lume" (IFCTEXT)
    IP = "65" (IFCTEXT)
    Localização = "Caxias do Sul - RS / Brasil" (IFCTEXT)
    Modelo = "ARC10W" (IFCTEXT)
    Nome do tipo = "ARC10W" (IFCTEXT)
    Número OmniClass = "23.80.70.14.11.17" (IFCTEXT)
    Peso = "0" (IFCTEXT)
    Título OmniClass = "Wall or Ceiling Mounted External Lighting" (IFCTEXT)
    URL = "https://www.powerlume.com.br/" (IFCTEXT)
    URL do produto = "https://www.powerlume.com.br/produtos/arandela-facho-dupla-concreto" (IFCTEXT)
    Vida útil = "60000h" (IFCTEXT)
  Materiais e acabamentos | properties | on 1 type object
    Frame = "Concreto, leve" (IFCTEXT)
    Refletor = "Metal - Alumínio" (IFCTEXT)
  Dados | properties | on 1 type object
    Versão = 1 (IFCINTEGER)
  Elétrica | properties | on 1 type object
    Comentários de voltagem = "110 ou 220Vac 50/60Hz com driver incorporado" (IFCTEXT)
    Lâmpada = "Placa LED" (IFCTEXT)
  Cotas | properties | on 1 type object
    Altura = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Largura = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Profundidade = 135. (IFCLENGTHMEASURE) [MILLI METRE]